ZOOM H1essential Description (for screen reader users)

Please place the unit on a table with the side that has many buttons face up. Turn the unit so that the end with the two XY mics is pointed away from you.

# Front (far end)

## Built-in XY mic

# Top

Parts are in the following order from the far end to the near end.

## Display

## Row of 4 rectangular buttons

## 2 pairs of smaller round buttons on the left and right of a central round button that feels slightly lower (we will call this “the 5 round button group”)

The functions of the 4 rectangular buttons in a row depend on the screen (mode)

### On the recording/recording standby screen, the button functions from left to right are:

#### Switch stereo/mono

#### Switch low cut on/off

#### Add mark (disabled when recording paused)

#### Move file being recorded (or most recently recorded file) to trash

### On the playback screen, the button functions from left to right are:

#### File options

#### Move back 3 seconds

#### Move forward 10 seconds

#### Move the file being played to the trash

### On the menu screen, the button functions from left to right are:

#### Go back

#### Move selection up

#### Move selection down

#### Open menu or confirm item

### On the File List Screen, the button functions from left to right are:

#### File options

#### Move selection up

#### Move selection down

#### Move file to trash

The 5 round button group has the following functions.

### The larger middle button starts and stops recording.(The small indentation above it is a recording indicator.)

### The upper left button stops recording and playback.

### The upper right button pauses and resumes recording and also starts, pauses and resumes playback of recorded files.

### The lower left button, when playing or paused, moves to the beginning of the file or the previous mark.When already near the beginning of a file, this opens the File List Screen.Pressing and holding it will search backward.

### The lower right button, when playing or paused, moves to the next mark.If there is no mark, this opens the File List Screen.Pressing and holding it will search forward.

# Left side

Parts are in the following order from the far end to the near end.

## Headphone/line output jack (stereo mini)

## Speaker/headphone volume dial

## Power switch (Slide this toward you completely to turn the power on or off. Slide this toward the mic end until it clicks into place to disable all button functions. This is called the hold function.)

## The opening at the near corner is for attaching a strap.

# Right side

Parts are in the following order from the far end to the near end.

## Mic/line input jack (stereo mini)

## USB Type-C port

## Menu button

## microSD card slot cover (A fingernail can be used with a notch at the top to open the cover from top to bottom. When inserting a microSD card, please orient the edge with the indentations toward the microphone end so that the side with the terminals is facing down. Insert it until it clicks into place. Press the card in again to eject it.)

# Back

Please turn the unit over. Parts are in the following order from the far end to the near end.

## Built-in speaker (many small holes)

## Screw hole (1/4-inch) for attaching a tripod

* Battery cover (Pull the tab in the middle away from the mics to open it. Use 2 AAA batteries. Install the batteries with their negative ends facing the springs. When reattaching the battery cover, insert the two small tabs on it in the indentations in the near end of the battery compartment. Then press the far end of the cover in until it clicks into place.)

© 2024 ZOOM CORPORATION Z2I-5220-02